## GWInstek GDS 2000E Series Instrument Driver Readme

#### 1. Overview

Instrument Driver Technology: LabVIEW Plug and Play (project-style)
Supported Language(s): LabVIEW
Supported Model(s):GWInstek GDS2072E, GDS2074E, GDS2102E, GDS2104E, GDS2202E, GDS2204E
Model(s) Tested: GDS2074E
Interface(s): USB, Ethernet
Firmware Revision(s) Tested: V1.03
Certified: Yes
NI Supported: Yes
Source Code Available: Yes
Driver Revision: 1.01
Original Release Date: 02/06/2015
Current Revision Date: 13/07/2015

#### 2. Required Software

Some software components need to be installed before using this instrument driver. The minimum versions of these components are listed below, and can be downloaded from the Download Site.
VISA 5.0.2 or later
Refer to the LabVIEW Help for more information about software requirements. You access the LabVIEW Help by selecting Help»Search the LabVIEW Help.

#### 3. Known Issues

To report issues or provide feedback about this instrument driver, please send an email to instrument.drivers@ni.com. 1. Self-test function is not supported at this time.

#### 4. Revision History

The latest version of this and other LabVIEW and LabWindows/CVI instrument drivers can be downloaded at the Instrument Driver Network.
REV 1.02, 11/06/2015
Modified by: GWInstek
Modified VIs:
- Configure Channel.vi: Add 25X and 250X in the Probe Attenuation Control .
REV 1.01, 07/13/2015
Modified by: GWInstek
Modified VIs:
- GWInstek GDS2000E Series Get Time Automeasure.vi: Remove Y axis display amplitude.
- Autosetup.vi:Replace VISA read .
REV 1.0, 2/04/15
Modified by: GWInstek
Original release.