USB-API and USB Driver(WinUSB) for GW PLR Series


Folder
Win_USBDriver      : USB Driver and Access API for PLR Series
_Define_USB_Source : Define USB API Access for VisualBasic.net and Visual C#
Sample_Application : Control Sample Program for Excel-VBA, Sequence Setting Application


Setup USB driver to 32bit Windos7 or higher.
 Login the Administrative Accunt.
 Execute All Windows update.
 Execute GWInstek_API32.msi.
 Execute Setup32.exe as Administratior (on the right mouse button clicked).
 The PLR Series set to USB mode and system address = 1 & PC address = 1(or other).
 Connect the PLR to PC via USB.
 Reinstall the USB Driver for PLR at Device manager, if the PLR is not recognized.


Setup USB driver to 64bit Windos7 or higher.
 Login the Administrative Accunt.
 Execute All Windows update.
 Execute GWInstek_API64.msi.
 Execute Setup64.exe as Administratior (on the right mouse button clicked).
 The PLR Series set to USB mode and system address = 1 & PC address = 1(or other).
 Connect the PLR to PC via USB.
 Reinstall the USB Driver for PLR at Device manager, if the PLR is not recognized.


USB Configuration  VID:2184/PID:0054/Vender Class
